# Chanora Software Architecture Description

**Lifecycle:** SWE.2 Software Architectural Design  
**Document status:** DV meeting baseline candidate  
**Date:** 2026-05-29  
**Direct upstream source:** `docs/srs.md`  
**Related system allocation:** `docs/sysdes.md`

## 1. Purpose

This Software Architecture Description defines Chanora's software architecture for DV review. It bridges SRS software requirements to SWE.3 detailed design and to SWE.5/SWE.6 verification planning.

This baseline captures the architecture visible in the current repository. It is sufficient for DV traceability review, while deeper per-module algorithms remain in `docs/architecture/sdd.md` and source-level design.

## 2. Architectural Scope

Chanora is a Flutter application with a Rust core. Flutter owns the user-facing shell, Material 3 widgets, localization, permission UX, and platform service presentation. Rust owns connection orchestration, protocol isolation, audio processing, storage coordination, diagnostics, server resolution, prefetch policy, and bridge DTOs.

## 3. Upstream SRS Allocation

| SRS group | Architectural allocation |
|---|---|
| SRS-003, SRS-008 through SRS-016 | Cross-platform app shell, Flutter UI, Rust core, platform adapters |
| SRS-017 through SRS-030 | Flutter UI, state presentation, connection and voice controls |
| SRS-031 through SRS-035 | Bridge layer and typed DTO boundary |
| SRS-036 through SRS-043 | Rust core connection lifecycle and state behavior |
| SRS-044 through SRS-053 | Protocol adapter and TeamSpeak-compatible server boundary |
| SRS-054 through SRS-061 | State synchronization and replay/reducer verification hooks |
| SRS-062 through SRS-083 | Audio subsystem, DSP, codec, PTT, mute/deaf, metering |
| SRS-084 through SRS-095 | Storage, secure storage, identity, diagnostics-sensitive data |
| SRS-096 through SRS-102 | Diagnostics, export, redaction, troubleshooting hooks |
| SRS-103 through SRS-123 | Platform adapters, packaging, release behavior |
| SRS-124 through SRS-143 | Verification support, analysis requirements, traceability rules |
| SRS-144 through SRS-184 | Material 3, adaptive UI, accessibility, localization, Unicode, app initialization |
| SRS-185 through SRS-218 | Platform baselines, PTT capability, transmit mode, no automatic telemetry, benchmark advisory |

## 4. Component Architecture

| Component | Repository location | Responsibility | Direct architectural dependencies |
|---|---|---|---|
| Flutter app shell | `apps/chanora_flutter/lib/main.dart`, services, widgets | App startup, screen composition, user actions, localization, Material 3 UI | Generated Rust bridge, platform plugins, Flutter services |
| Flutter service layer | `apps/chanora_flutter/lib/services/` | Permission flows, lifecycle policy, host prefetch debounce, link trust, state mapping, platform back intent | Flutter app shell, generated bridge APIs, platform plugins |
| Flutter widget layer | `apps/chanora_flutter/lib/widgets/` | Connect UI, channel tree, chat, voice controls, settings, diagnostics surfaces | Flutter services, generated DTOs, design tokens |
| Bridge layer | `crates/chanora_bridge`, `apps/chanora_flutter/lib/src/rust/` | Typed Flutter/Rust boundary and generated bindings | Rust core, Flutter generated code |
| Rust core | `core/chanora_core` | Connection lifecycle, orchestration, reconnect behavior, storage coordination, voice state | Protocol, audio, storage, diagnostics, state, resolver/prefetch |
| Protocol adapter | `crates/chanora_protocol` | Isolate `tsclientlib`, expose typed protocol DTOs/errors | Rust core, external compatible server |
| State sync | `crates/chanora_state` | Snapshot/delta model, channel join helpers, reducer behavior | Rust core, protocol DTOs |
| Audio subsystem | `crates/chanora_audio` | Capture/playback, Opus, DSP, PTT, voice activity reservation, platform units | Rust core, platform APIs, protocol audio path |
| Storage | `crates/chanora_storage` | Bookmarks, identities, encrypted local data, platform keyring integration | Rust core, platform secure storage |
| Diagnostics | `crates/chanora_diagnostics` | Redaction, log sink, export bundle, known-secret registry | Rust core, Flutter diagnostics UI |
| Server resolver | `crates/chanora_resolver` | SRV/TSDNS/DNS fallback resolution | Rust core, prefetch crate |
| Server prefetch | `crates/chanora_server_prefetch`, Flutter `prefetch_debouncer.dart` | Invisible host-field resolution warming, TTL cache, generation safety | Resolver, Flutter connect UI, Rust core |

## 5. Static Architecture View

```text
Flutter UI/widgets/services
  -> generated Dart bridge API
  -> chanora_bridge
  -> chanora_core
      -> chanora_protocol -> tsclientlib -> external compatible server
      -> chanora_state
      -> chanora_audio -> platform audio APIs / Opus / DSP
      -> chanora_storage -> platform secure storage / SQLite
      -> chanora_diagnostics
      -> chanora_server_prefetch -> chanora_resolver -> network DNS/TSDNS
```

The bridge is the trust and type boundary between Flutter and Rust. Flutter must not directly depend on protocol-library internals. Rust core must not expose platform-specific storage or audio details to UI code except through stable DTOs and capability fields.

## 6. Runtime Flow Architecture

### 6.1 Connect Flow

```text
User enters host/bookmark
  -> Flutter connect widgets
  -> optional prefetch debounce
  -> bridge connect command
  -> Rust core supervisor
  -> resolver / prefetch cache
  -> protocol adapter
  -> external compatible server
  -> state snapshot/events
  -> bridge event stream
  -> Flutter state mapper and widgets
```

### 6.2 Voice Flow

```text
Microphone / platform input
  -> audio capture unit
  -> DSP chain: HPF, NS, AEC, AGC where active
  -> PTT/mute/transmit gate
  -> Opus encode
  -> protocol adapter
  -> external compatible server

External server voice
  -> protocol adapter
  -> jitter/decode path
  -> mixer / per-user controls
  -> platform output
```

### 6.3 Diagnostics Flow

```text
Runtime event or error
  -> diagnostic log sink / known-secret registry
  -> redactor
  -> user-initiated export bundle
  -> Flutter share/export surface
```

## 7. Interface Catalogue

| Interface | Producer | Consumer | Architectural rule |
|---|---|---|---|
| Bridge command DTOs | Flutter generated API | `chanora_bridge`, Rust core | Stable typed DTOs; no raw protocol-library types cross to Flutter |
| Bridge event DTOs | Rust core / bridge | Flutter services/widgets | User-safe errors and capability fields are explicit |
| Protocol DTOs | `chanora_protocol` | Rust core, state sync | Protocol adapter isolates `tsclientlib` |
| Audio configuration | Flutter settings / Rust core | `chanora_audio` | Voice modes and processing flags are explicit; VAD remains disabled/deferred |
| Storage records | Storage crate | Rust core / Flutter UI via bridge | Secrets stay behind secure-storage abstraction |
| Diagnostic bundles | Diagnostics crate | Flutter diagnostics UI | Redaction runs before export or display |
| Platform capability records | Platform adapters/audio/PTT backends | UI and release record | UI/release wording must not over-claim capability |

## 8. Dependency Rules

| Rule | Rationale |
|---|---|
| Flutter UI depends on generated bridge APIs, not Rust internals | Keeps UI stable across Rust implementation changes |
| Rust core orchestrates crates but protocol/audio/storage crates remain separately testable | Supports SWE.4 unit verification and bounded responsibilities |
| Protocol adapter is the only component that owns `tsclientlib` coupling | Protects the app from protocol-library leakage |
| Diagnostics redaction must be reusable by runtime logging and export | Prevents split redaction behavior |
| Platform-specific behavior stays in platform adapters or audio platform units | Keeps cross-platform logic testable and reduces conditional sprawl |
| Release claims consume capability records and release evidence | Prevents over-claiming PTT, signing, packaging, or secure-storage behavior |

## 9. Non-Functional Allocation

| Concern | Architectural mechanism | Verification owner |
|---|---|---|
| Real-time audio responsiveness | Rust audio subsystem, benchmark advisory, bounded callback behavior | Audio / Platform QA |
| Privacy and no automatic telemetry | User-initiated diagnostics, no automatic upload policy | Security / Privacy QA |
| Secure secret handling | Platform secure-storage abstraction and encrypted local storage | Security / QA |
| Cross-platform UI | Flutter Material 3, design tokens, responsive widgets | Software QA / UX |
| Protocol compatibility | `tsclientlib` adapter isolation and compatible-server matrix | Protocol / Integration QA |
| Release reproducibility | CI, build scripts, artifact hashes, release-readiness record | Release / Operations QA |

## 10. Architectural Decisions Captured by This Baseline

| Decision | Architectural outcome |
|---|---|
| Flutter + Rust split | Flutter owns presentation; Rust owns protocol/audio/storage/diagnostics core behavior |
| `tsclientlib` isolation | Protocol compatibility is behind `chanora_protocol` |
| Secure storage abstraction | Platform storage details do not leak into UI or unrelated crates |
| Advisory audio benchmarks | Performance regressions are surfaced without making CI a hard release gate at this stage |
| PTT capability levels | Platform PTT support is represented as capability data and must match release wording |
| VoiceActivity deferral | `VoiceActivity` remains reserved/disabled until a later baseline allocates implementation |
| No automatic diagnostic upload in MVP | Diagnostics are local and user-initiated unless future approved requirements change policy |

## 11. Verification Handoff

| Verification plan | SAD handoff |
|---|---|
| SWE.4 | Component boundaries define unit-test ownership for Flutter services/widgets and Rust crates |
| SWE.5 | Interface catalogue and runtime flows define integration paths |
| SWE.6 | SRS allocation and acceptance flows define software acceptance evidence |
| SYS.4 | Platform capability and external-server boundaries define system integration evidence |

## 12. Traceability to SRS

This SAD derives only from `docs/srs.md`. The broad SRS group-to-component allocation in section 3 is the controlling SWE.2 trace for DV. Detailed item-level trace is represented by the SRS coverage matrix and `docs/governance/traceability-matrix.md`.

## 13. Open Architecture Risks

| Risk | Impact | Control |
|---|---|---|
| SAD item numbering from historical status references is not reconstructed in this baseline | Existing references such as `SAD-043` and `SAD-046` are not itemized here | Treat this as a DV baseline SAD; add itemized SAD IDs in a follow-up if process requires strict ID-level review |
| Some architecture views are textual rather than C4 diagrams | Reviewers may request visual C4 views | Record as documentation hardening, not a blocker for DV baseline if textual views are accepted |
| Release/platform architecture evidence is incomplete | Public release remains blocked | Controlled by release-readiness and waiver records |

## 14. DV Conclusion

This SWE.2 baseline is sufficient to remove the missing-SAD traceability gap for DV review. It does not replace candidate test evidence or final release approval.
